Input CAN Message

The Seat Belt Reminder module must check the following data:

* Operation Mode
* Vehicle Speed
* Distance traveled
* Engine status
* Driver Front Door switch status
* Chime active status
* Buckle switch status
* occupancy status

Output CAN Message

The Seat Belt Reminder shall send the following data:

* CAN messages to control the chime
* CAN messages to control the driver reminder telltales.
* CAN messages to control the passenger reminder telltales.
* CAN messages to command DIC.